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SaFETY PRECAUTIONS

Thank you for purchasing ABTS-K5:
This is your assurance of quality performance and value. Our engineers have included many useful and convenient features in this product. Please be sure to read this instruction Manual completely to make sure you are getting the maximum benefit from each feature.

This product was manufactured using the highest quality components and standards of workmanship.
It was tested by inspectors and found to be in perfect working order before it left our factory.

TO PREVENT FIRE OR SHOCK HAZARD DO NOT EXPOSE THIS APPLIANCE TO RAIN OR MOISTURE.
Notes: ━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━
· The images appearing in this manual are for reference only.
· Due to continual revision and improvement on our products design and specifications are subject to change without further notice.

CHARGEr AND BATTERY 

BATTERY CHARGE INDICATOR

[image: C:\Users\Administrator\Desktop\8787\DK-12 说明书.jpgDK-12 说明书]      LED panel has battery status indicator. In the middle of 
the shape of the battery has four horizontal lines, each 
horizontal line represents 25% of electricity remaining. 
      When no horizontal line in the shape of the battery or 
the shape flashes, please power of and promptly 
charge to avoid damage to the battery.
      When charging, the battery indicator on LED display
 panel flashes. 
      The indicator stops blinking after full charged. Then 
please continue to charge the battery for 1-2 hours to 
extend the battery life.



WARNING!

      If the battery is under voltage, please fully charge it within 48 hours.
If the speaker has to be left unused for a long time, please let the battery fully charged, otherwise it will cause damage to the battery.



TECHNICAL SPECIFICATION

MODEL                                     ABTS-K5
     Rated Power:                                 ≤30W
     Input sensitivity:                               450±50mV
Battery:                                      7.4V 4000mAh
DC 5V IN:                                    DC 5V 
     Charging time:                                4-6h
     Working time:                                 3-6h
[bookmark: OLE_LINK1]Frequency response:                          20Hz-20KHz
     Audio S/N:                                    ≥71dB
     Bluetooth version:                              5.0
     Bluetooth channel emission power:              2dbm
     Bluetooth frequency:                           2.4 – 2.483GHz

DESCRIPTION OF REMOTE CONTROL
[image: C:\Users\Administrator\Desktop\8787\QQ截图20190619175845.jpgQQ截图20190619175845][image: C:\Users\Administrator\Desktop\8787\1.jpg1]                                           MUTE
Mute or restart the speaker.

INPUT (INPUT SELECTION)
Input selection (AUX input / Bluetooth / USB / FM function).

VOL+ (INCREASE VOLUME)

PLAY /PAUSE/SCAN

PREVIOUS

VOL-(DECREASE VOLUME)

NEXT

LED LIGHT CONTROL
Turn on the light / change the light mode.
Long press to turn off the light.

REPEAT
Repeat one, repeat all, repeat folder.

RECORD/PLAY RECORDING
Start recording, long press it to play the recordings.

PREVIOUS FOLDER
Change to the previous folder on USB input mode.

NEXT FOLDER
Change to the next folder on USB input mode.
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DESCRIPTION OF CONTROLs
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DC 5V charging interface (for adaptor).

USB PLAY SLOT

VOLUME

INPUT[image: ] 
With a short press on the button, select the input mode (AUX input / Bluetooth/ USB / FM radio) 

G-BASS 
Super good bass button.

LED LIGHT CONTROL 	
Short press to change the light mode.

NEXT [image: ]









PLAY / PAUSE / SCAN [image: ]

PREVIOUS[image: ]

MENU
With a short press on the button, adjust treble /
bass / microphone volume / microphone echo /
guitar volume.

MIC / GUITAR SLOT
Use to connect the microphone / guitar jack.

GUITAR
Press to enter guitar mode.

AUX INPUT

POWER
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MICROPHONE CONTROLS AND BASIC OPERATION
[image: C:\Users\Administrator\Desktop\8787\QQ截图20190619160226.jpgQQ截图20190619160226]WIRELESS MICROPHONE




[image: C:\Users\Administrator\Desktop\8787\1.jpg1]                                           MICROPHONE ON/OFF
[image: C:\Users\Administrator\Desktop\8787\2.jpg2]                                                 MUTE
[image: C:\Users\Administrator\Desktop\8787\3.jpg3]                                                 LIGHT INDICATOR
Microphone frequency:                         201.6 MHz
Channel emission power for wireless microphone:  50mW
FUNCTIONS 
RECORDING FUNCTION                     FM FUNCTION
[image: C:\Users\Administrator\Desktop\8787\QQ截图20190621110251.jpgQQ截图20190621110251]Choose INPUT to switch to FM RADIO.

Search and tune automatically to radio 
stations by pressing     on the remote control ro long press the    button on the speaker.
Switch channels, by pressing      and      on     the speaker or the remote control. 
Press      to record the voice into the external memory like USB disk on the speaker.

If the external memory is first time used, the system will automatically built a new folder named VOICE, and recording files in it will be named REC001, REC002, and so on.

In record mode, press      / INPUT to stop recording.

Long press“  “ to play the recordings in the external memory, press PREV and NEXT to choose the recordings to play.
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AWS FUNCTION (AKAI WIRELESS STEREO)
1、 [image: C:\Users\Administrator\Desktop\8787\QQ截图20190621110301.jpgQQ截图20190621110301]Select the Bluetooth mode on the 2 speakers you wish to pair.
2、The 2 speakers need to be exactly the same in order to pair under AWS mode.
3、Select any one of the speakers and long press the "NEXT" button.
4、 A sound will be heard and the main speaker display will indicate "HOST" confirming that the 2 speakers are now paired.
5、The speaker display should indicate "BT".
6、To disconnect the AWS function, simply press the "PREVIOUS" button on the main speaker.
7、The speaker display should indicate "BT" in a flashing mode.
8、Long press the button to completely disconnect the Bluetooth connection with your mobile 
device.
BLUETOOTH OPERATION
IMPORTANT:
Prior to use Bluetooth function, your speaker should be paired firstly with your Bluetooth device.
(“Paring” means establish connection between Bluetooth devices such as MOBILE PHONE, TABLETS,
 PC, ETC).
[image: ]
1. Press the BT MODE button to switch into 
the BT MODE (Bluetooth mode).
(fig.1)

2. In BT MODE, a sound indication will
announce that Bluetooth pairing 
mode is ready.
Then the micro system will search 
automatically for Bluetooth devices.

3. Turn on Bluetooth functionality on 
your device and make it discoverable 
(See your devices instructions to add 
or setup a Bluetooth device).
4. Search for Bluetooth equipment:
ABTS-K5 is your speaker identification.
(fig.2)
A sound indication will announce that Bluetooth 
devices are successfully paired. (During the pairing, 
if a password is required, you need to input code “0000”).
Your Bluetooth device stores the speaker unique identification at the same time.

ACCESSORIES

· 1 Charging cable
· 1 remote control
· 1 wireless microphone



TROUBLE SHOOTING GUIDE

If a fault occurs, first check the points listed below before taking the speaker to repair.
Do not open the speaker as there is risk of electric shock.
If you are unable to remedy a problem by following these hints, consult your dealer or service center.

	SYMPTOM
	CAUSE
	CORRECTION

	Sound

	No sound
	No input sound source.
	Use a better music signal.

	
	Volume is too low.
	Adjust volume.

	Distortion of sound
	Volume too high.
	Turn down the volume.

	
	Speaker may be damaged.
	If speaker is damaged, repair or replace it.

	Karaoke

	Karaoke does not work
	Microphone plug is not fully inserted.
	Plug microphone properly into the socket.

	
	Microphone switch is not on.
	Turn on microphone switch.

	
	Microphone volume knob is at the lowest position.
	Adjust microphone volume properly.

	
	Wireless microphone has low battery.
	Replace battery.

	MP3

	MP3 does not play
	The song format in the USB disc is incorrect.
	Transform song format into MP3 format.

	
	Improper operation has caused a process disorder.
	Reboot the machine.

	
	USB disk is disconnected.
	Insert USB disc properly.

	Remote control

	The remote control does not work properly
	The remote control is too far from the unit.
	Operate the remote control within about 6m.

	
	There is an obstacle in the path of the remote control and the unit.
	Remote the obstacle.

	
	The battery in the remote control is exhausted.
	Replace the battery with new one.





WARNING!
Under no circumstances should you try to repair the set yourself, as this will invalidate the warranty.

DISPOSAL OF ELECTRICAL AND ELECTRONIC EQUIPMENT

[image: WEEE marking logo]This symbol on the product or packaging means that the product should not be treated as household waste. Do not throw garbage at the end of its life, but take it to a collection center for recycling. in this way you will help to protect the environment and be able to prevent any negative consequences that it would have on the environment and human health.
To find your nearest collection center:
·  Contact local authorities
· Access the website: www.mmediu.ro 
Request additional information from the store where you purchased the product.




IMPORTATOR: INTERVISION TRADING-RO SRL
Bld. I.C Bratianu, nr. 48-52, corp A, etaj. 5,
camera 504-505, oras Pitesti, judet Arges, Romania
Cod postal: 110121
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