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MULTIMEDIA SPEAKER SYSTEM

EN - ENGLISH
REMOTE CONTROL
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	1. STANDBY: Press this button to Turn On/Turn Off the Set.

2. INPUT: Press this button to select Input (Aux/FM/BT/USB/SD).

3. USB: USB Audio Play.

4. SD: SD Audio Play.

5. FM: Play FM Station.

6. AUX IN: AUX Audio Input.

7. TREBLE (-): To reduce treble of the sound.

8. TREBLE (+): To increase treble of the sound.

9. BASS(-): To decrease the bass in the sound.

10. BASS (+): To increase the bass in the sound.

11. ST(-): To go to Previous FM Station.

12. ST(+): To go to Next FM Station.

13. PREV: In USB/SD Mode – to play previous song. In FM Mode – to go to previous radio station.

14. NEXT: In USB/SD Mode – to play next song. In FM Mode – to go to Next Radio Station.

15.  VOL(-) To decrease the master volume.

16. VOL(+) To increase the master volume.

17. PL/PA/MUTE: To operate function of Play/Pause or to Mute the sound.

18. FT(-): FM Tuning Decreases by 0.1 MHZ by each Press.

19. FT(+): FM Tuning Increases by 0.1MHZ by each Press.

20. 0-9: to choose the song number in USB/SD Mode.

21. REPEAT FUNCTION

ONE: Repeat current song.

ALL: Repeat all songs.

SHUF: Shuffle the songs and play again and again.

OFF: Play every song once, use their order.

22. SEARCH: FM Station Auto Scan only.


REMARK
1. Do not expose the apparatus to high temperature, water, moisture.

2. Do not attempt to disassemble the product to avoid electric shock; only professionals should perform service.

3. Please turn off the power and pull out the plug when you don’t use this product.

CONTROL PANEL DIAGRAM
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	(1) LED display

(2) Volume/Mode adjustment

(3) MODE

(4) Play/Pause

(5) SD Card Slot

(6) USB input

(7) Previous/FM scan

(8) Next/FM scan


	SPEAKERS
	
	
	
	AMPLIFIERS
	

	
	SATELLITE SPEAKER
	SUBWOOFER
	
	Channel Separation
	45 db

	Driver Size
	3 inch
	8 inch
	
	Signal to Noise Ratio
	68 db

	Impedance
	4 Ω
	8 Ω
	
	Power Requirements
	

	Frequency Range
	35Hz-20KHz
	
	
	Voltage

Frequency 
	220-230V~

50Hz


BACK PANEL CONNECTION DIAGRAM
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DISPOSAL OF ELECTRICAL AND ELECTRONIC EQUIPMENT
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This symbol on the product or packaging means that the product should not be treated as household waste. Do not throw garbage at the end of its life, but take it to a collection center for recycling. in this way you will help to protect the environment and be able to prevent any negative consequences that it would have on the environment and human health.

To find your nearest collection center:

-Contact local authorities

- Access the website: www.mmediu.ro

Request additional information from the store where you purchased the product.
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MANUALUL UTILIZATORULUI

SISTEM MULTIMEDIA
RO - ROMANA
TELECOMANDA
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	1. STANDBY: Apasati acest buton pentru a porni/opri aparatul.

2. INTRARE: Apasati acest buton pentru a selecta modul de intrare (Aux/FM/BT/USB/SD).

3. USB: Redare automata prin USB.

4. SD: Redare audio de pe card SD.

5. FM: Reda postul FM.

6. AUX IN: Intrare audio AUX.

7. INALTE (-): Reduce sunetele inalte.

8. INALTE (+): Mareste sunetele inalte.

9. BASS(-): Reduce bass-ul din sunet.

10. BASS (+): mareste bass-ul din sunet.

11. ST(-): Trece la postul FM anterior.

12. ST(+): Trece la postul FM urmator.

13. PREV: In modul USB/SD – pentru a reda melodia urmatoare. In modul FM -  pentru a trece la postul de radio anterior.

14. NEXT: In modul USB/SD – pentru a reda melodia urmatoare. In modul FM – pentru a trece la urmatorul post de radio.

15.  VOL(-) pentru a micsora volumul principal.

16. VOL(+) pentru a mari volumul principal.

17. PL/PA/MUTE: pentru a opera functia de redare/pauza sau pentru a opri sunetul.

18. FT(-): Cautarea FM scade cu cate 0.1 MHZ la fiecare apasare.

19. FT(+): Cautarea FM scade cu cate 0.1MHZ la fiecare apasare.

20. 0-9: pentru a alege numarul cantecului in modul USB/SD.

21. FUNCTIA REPEAT

UNU: Repeta melodia curenta.

TOATE: Repeta toate melodiile.

SHUF: Amesteca melodiile si le reda tot timpul.

OPRIT: Redati fiecare melodie o data, in ordine.

22. CAUTARE: Scanare automata a posturilor FM.


OBSERVATIE
1. Nu expuneti aparatul la temperaturi inalte, apa, umezeala.

2. Nu incercati sa demontati produsul pentru a evita electrocutarea; doar personalul calificat trebuie sa efectueze lucrari de service.

3. Opriti alimentarea si scoateti cablul din priza atunci cand nu utilizati acest produs.

DIAGRAMA PANOU CONTROL
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	(1) LED afisaj

(2) Reglare volum/mod

(3) MOD

(4) Redare/Pauza

(5) Slot card SD

(6) Intrare USB

(7) Anterior/scanare FM

(8) Urmator/scanare FM


	DIFUZOARE
	
	
	
	AMPLIFICATOARE
	

	
	DIFUZOR SATELIT
	SUBWOOFER
	
	Separare canale
	45 db

	Diametru difuzor
	3 inch
	8 inch
	
	Raportul semnal zgomot
	68 db

	Impedanta
	4 Ω
	8 Ω
	
	Energie necesara
	

	Marime frecventa
	35Hz-20KHz
	
	
	Voltaj

Frecventa 
	220-230V~

50Hz


DIAGRAMA CONECTARE PANOU SPATE
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Reciclarea echipamentelor electrice şi electronice uzate:

Acest simbol prezent pe produs sau pe ambalaj semnifică faptul că produsul respectiv nu trebuie tratat ca un deşeu menajer obişnuit. Nu aruncaţi aparatul la gunoiul menajer la sfârşitul duratei de funcţionare, ci duceţi-l la un centru de colectare autorizat pentru reciclare. În acest fel veţi ajuta la protejarea mediului înconjurător şi veţi putea împiedica eventualele consecinţe negative pe care le-ar avea asupra mediului şi sănătăţii umane.

Pentru a afla adresa celui mai apropiat centru de colectare:

-         Contactaţi autorităţile locale;

-         Accesaţi pagina de internet: www.mmediu.ro ;

-         Solicitaţi informaţii suplimentare de la magazinul de unde aţi achiziţionat produsul.
